(footprint "CPG1316S01D02"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.05 5.55 0)
		(unlocked yes)
		(layer "Cmts.User")
	)
	(property "Value" "CPG1316S01D02"
		(at 0 9 0)
		(unlocked yes)
		(layer "Cmts.User")
		(hide yes)
	)
	(property "Footprint" ""
		(at 0 10.85 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_circle
		(center -5.8 2.75)
		(end -5.3 2.75)
		(fill none)
		(layer "Edge.Cuts")
	)
	(fp_circle
		(center 5.8 -2.75)
		(end 6.4 -2.75)
		(fill none)
		(layer "Edge.Cuts")
	)
	(fp_text user "17 spacing"
		(at -0.025 -7.5 180)
		(layer "Dwgs.User")
	)
	(fp_text user "switch"
		(at -0.07 -5.66 0)
		(layer "Eco1.User")
	)
	(fp_text user "keycap"
		(at -2.5 7.5 0)
		(unlocked yes)
		(layer "Eco2.User")
	)
	(pad "1" smd rect
		(at -2.5 2.65)
		(size 1.55 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "2" smd rect
		(at 2.5 2.65)
		(size 1.55 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "MP" smd rect
		(at -6.35 -6)
		(size 2 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "MP" smd rect
		(at -6.35 6)
		(size 2 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "MP" smd rect
		(at 6.35 -6)
		(size 2 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(pad "MP" smd rect
		(at 6.35 6)
		(size 2 2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(thermal_bridge_angle 45)
	)
	(model "/home/idank/dev/keyboards/idank-kicad-lib/PG1316S.STEP"
		(offset
			(xyz -4.75 -6.25 -10.25)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
